RME Intelligent Audio Solutions

MADIface XT / XT II / USB / Pro, Fireface UFX+ / UFX II / UFX III, OctaMic XTC, ADI-2 Pro/AE/FS/DAC, ADI-2/4 Pro, Digiface USB / AVB / AES / Dante / Ravenna, USB.IO

Driver for Windows 10 / 11, Intel x64 and Arm

Important information: Driver version 1.0.14


Installation
-------------

Latest firmware
https://www.rme-audio.de/downloads/fut_madiface_win.zip

The firmware update is not possible unless the driver had been installed before.

Follow the instructions of the RME Driver Install Wizard. This tool installs/updates all driver files. In most cases, a restart is no longer necessary. If required the installer will notify you.


----------------------

News, changes and fixes

Attention:

- This driver requires Windows 10 (1709) or higher

- This driver does not support 32 bit Windows OS anymore (32 bit apps can still be used with an x64 system)

- This driver also supports Windows 11 Arm systems. Both WDM and ASIO are available. ASIO is included as 32 bit and 64 bit, both Arm64EC and Arm native.

- The installer is completely reworked and now copies current files to C:\Program Files\RME\MADIface

- Changing between the former and this driver on Intel systems, back and forth, should be easy and without issues 

- Some audio apps on Arm might require to set the power mode not to Best Performance, but Best Power Efficiency, to be able to use latencies below 1024 samples. This might be true only for low CPU apps, though, and needs further investigation, but in any case the driver has no influence on this. As an example, on current computers Reaper and Cubase need about 256 sample buffer size for a fully click-free operation.

- In most cases, a restart is no longer necessary after both initial installation and update. TotalMix FX and Settings dialog are immediately available in the notification area and are also updated.

- To completely uninstall the driver start rmeinstaller.exe and choose Uninstall. Note: Uninstall via Windows Apps (Add & Remove) is no longer supported.


---------------------

V 1.0.14 (01/16/2026)

- Enables the current Windows FUT to flash Digiface USB and MADIface USB when in CC mode

---------------------

V 1.05 (09/08/2025)

- Fix WDM Settings Dialog MADIface XT / XT II: AES Input only became active when selecting Phones instead

---------------------

V 1.02 (05/05/2025)

No change to driver.

- Installer no longer locks the started apps

---------------------

V 1.02 (05/05/2025)

- Installer now includes the required VS runtimes

- Added MIDI I/O for USB.IO (requires new firmware for USB.IO)


New in TotalMix FX 1.99:

- Talkback routing not correct when Trim had been deactivated

- Fix crash when Talkback source was set back to None

- Added Aux devices for the HDSPe AoX (not relevant for the USB driver)


---------------------

V 1.0 (01/13/2025)

- Fix installer: TotalMix FX help was missing

- Added to the installer: New option to install the driver without TotalMix FX. This equals the older driver, which did not start TotalMix in case only (!) ADI-2 series devices were installed and used on the computer.

---------------------

V 1.0 (01/08/2025)

- Fix installer: Settings dialog can be called from an ASIO DAW again

- Fix installer: Driver installation is now also performed correctly for user accounts


New in TotalMix FX 1.98 x64:

- Eliminates crash when clicking on the playback button for channel selection (DURec)

- Channel status narrow in CRM is retained even if the CRM was minimized (CRM options not visible)

- HDSP9632 and HDSPe AIO: Check marks in the routing dialog now appear on all active channels

- HDSP9632 and HDSPe AIO: Switching off phones in the CRM (none) did not remove them from the CRM


---------------------

V 0.9849 (11/15/2024)

- 64 bit driver, compiled with latest Microsoft tools and using latest Microsoft guidelines 

- Reworked installer, now handles installation and uninstallation completely

- supports Intel x64 and Arm (ASIO native and Arm64EC)

- comes with TotalMix 1.97 (2)


----------------------


Copyright RME 01/2026
All rights reserved. Windows 10/11 are trademarks of Microsoft Corporation. ASIO is a trademark of Steinberg Media Technologies GmbH. ADAT is a trademark of the Alesis Corp. Arm is a registered trademark of Arm Limited.
